标题：Office Linear Light VACE LED 24W 30W 48W 60W Dimmable LED Linear Lighting

**roduct feature**

1. You can choose to be spliced ​​with a splicer, so that the lamps are no longer single and unchanged, and more shapes are waiting for you to discover
2. The length of the hanging wire is 150CM, which can easily adjust the height of the lamp
3. Made of well-known brand chips, safe and stable quality
4. Three color temperatures 3000K/4000K/6000K to choose from, bright lights make you more focused on work
5. The PC cover has an excellent light transmittance,providing you softer and more uniformlight
6. Thickened load-bearing hanging wire made of hardware, sturdy and thick, anti-corrosion and anti-rust, the hanging wire has strong tensile strength
7. Built-in constant current driver to ensure that the LED light source lamp beads work stably under constant current
8. The light housing is made of high quality aluminum alloy material,powder coating,corrorion resistance,easy to clean

The LED linear light is a high performance, flexible and modular profile system with recessed, surface, wall mounted andsuspended/pendant options. Stand-alone or continuous system configuration are available.

Indirect/Direct lighting is generally recommended for spaces with high (10+ feet) and white finished ceilings to allow the light to reflect back down into the space.

With carefully designed details, the basic luminaire shape allows the creation of infinite patterns. This highly adaptable linear light fixture adds character to office spaces, classrooms, conference rooms, supermarket and more.

Short description

1. Suitable for ceiling installation and hanging wire installation
2. Multiple width and length options
3. Can cusotmize the shape accordingly to your needs
4. Seamless connection
5. PC cover transmitting rate reach 86%, luminous reach 110lm/w.
6. IC driver. No flicker, No glaring.CIR ≥ 80.PF ≥ 0.9 and corrosion.
7. Built in driver,conforming to EMC
8. Aluminum material to make efficient heat dissipation

Product Spec.



8710303 24W 1920lm 1200\*60\*80 pendant/surface mounte

8710303 48W 3840lm 2400\*60\*80 pendant/surface mounte

8710313 30W 2400lm 1200\*75\*80 pendant/surface mounte

8710303 60W 4800lm 2400\*75\*80 pendant/surface mounte

CCT : 3000K/4000K/6000K

Lamp Luminous Efficiency(lm/w):80-100

IP Rating : IP20

Install style:Recessed

Optional Control : Triac/0-10V/1-10V/DALI

Operating temperature: -20℃-+40℃

Working Life : 30000H

Ouput voltage : 220-240V 50/60Hz

Transformer mounting: built in

Control : standard on/off

Housing Color : White/Black

Certificate : CE/CB

Warrenty : 3 years

Applications:office,school,corridor,shopping mall,rest area,gym

（以上显示要和上面参数信息那边，深浅底交替）

Application:office,school,corridor,shopping mall,rest area,gym